<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<library>
<description>1</description>
<packages>
<package name="TSSOP20">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 20&lt;/b&gt;&lt;p&gt;
MAX3223-MAX3243.pdf</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="DS1306">
<pin name="VCC2" direction="pwr"/>
<pin name="VBAT" direction="pwr"/>
<pin name="X1" direction="in"/>
<pin name="X2" direction="in"/>
<pin name="/INT0" direction="out"/>
<pin name="INT1" direction="out"/>
<pin name="1HZ" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="CE" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="SDO" direction="out"/>
<pin name="VCCIF" direction="pwr"/>
<pin name="32KHZ" direction="out"/>
<pin name="VCC1" direction="pwr"/>
<pin name="SERMODE" direction="in"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="DS1306" prefix="IC">
<description>Serial Alarm Real-Time Clock</description>
<gates>
<gate name="G$1" symbol="DS1306"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="/INT0" pad="5"/>
<connect gate="G$1" pin="1HZ" pad="7"/>
<connect gate="G$1" pin="32KHZ" pad="15"/>
<connect gate="G$1" pin="CE" pad="10"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="INT1" pad="6"/>
<connect gate="G$1" pin="SCLK" pad="11"/>
<connect gate="G$1" pin="SDI" pad="12"/>
<connect gate="G$1" pin="SDO" pad="13"/>
<connect gate="G$1" pin="SERMODE" pad="9"/>
<connect gate="G$1" pin="VBAT" pad="2"/>
<connect gate="G$1" pin="VCC1" pad="16"/>
<connect gate="G$1" pin="VCC2" pad="1"/>
<connect gate="G$1" pin="VCCIF" pad="14"/>
<connect gate="G$1" pin="X1" pad="3"/>
<connect gate="G$1" pin="X2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E" package="TSSOP20">
<connects>
<connect gate="G$1" pin="/INT0" pad="7"/>
<connect gate="G$1" pin="1HZ" pad="9"/>
<connect gate="G$1" pin="32KHZ" pad="18"/>
<connect gate="G$1" pin="CE" pad="12"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="INT1" pad="8"/>
<connect gate="G$1" pin="SCLK" pad="14"/>
<connect gate="G$1" pin="SDI" pad="15"/>
<connect gate="G$1" pin="SDO" pad="16"/>
<connect gate="G$1" pin="SERMODE" pad="11"/>
<connect gate="G$1" pin="VBAT" pad="2"/>
<connect gate="G$1" pin="VCC1" pad="20"/>
<connect gate="G$1" pin="VCC2" pad="1"/>
<connect gate="G$1" pin="VCCIF" pad="17"/>
<connect gate="G$1" pin="X1" pad="3"/>
<connect gate="G$1" pin="X2" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
